{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["工程量清单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"工程量清单","index":0,"n_rows":15,"n_cols":7,"rows_kept":15,"merged":[[0,0,0,6],[11,0,11,4],[12,0,13,6],[14,0,14,6],[15,0,15,6]],"flags":["formulas_cached_only"]}
["江苏东方水务有限公司供配电设施代维及运行管理服务工程量清单"]
["序号","名称","单位","数量","全费用综合单价(元)","合价(元)","维保年限"]
[1,"配电变压器(1250KVA/台)","台/年",4,null,null,"1年"]
[2,"高压配电柜","台/年",14,null,null,"1年"]
[3,"低压配电柜","台/年",23,null,null,"1年"]
[4,"直流屏及消防设施","台/年",1,null,null,"1年"]
[5,"高压电缆检测试验","根/年",6,null,null,"1年"]
[6,"母线","段/年",2,null,null,"1年"]
[7,"接地系统","系统/年",1,null,null,"1年"]
[8,"高压避雷器","组/年",2,null,null,"1年"]
[9,"安全工器具","项/年",1,null,null,"1年"]
["合计"]
["备注：                                                                                                                                            1、包含供配电设施的日常维护、保养及500元以内的配件更换等；                                                                                                    2、所有更换的配件需为原厂正品配件；                                                                                                                  3、对于甲方日常紧急报修，需在2小时内到现场，最迟24小时解决问题，特殊情况下需甲方同意延长时间；                                                 4、甲方将对维保单位进行考核，考核不通过，并进行处罚，直至扣除全部工程款；                                                      5、以上单价为全费用综合单价，包括人工费、材料费、机械费（含大型机械进退场费）、管理费、利润、税金、建筑规费、安全文明施工措施费、临时设施费、检验试验费等一切费用。"]
[]
["投标人（盖章）：                                \n日 期：           年        月       日\n"]